Activate Reservoir Operation in CaMa-Flood

15 April, 2024  
Dai Yamazaki and CaMa-Flood development team  
IIS U-Tokyo

In this document, the procedures to activate reservoir operation scheme in CaMa-Flood are explained.

Note: The format of dam parameter list file is slightly modified in v4.13 (fldsto/uparea parameter was excluded, construction year is added). Please use a dam parameter list which is generated by the updated script.

# Setting Reservoir Operation Parameters

First step of activating reservoir operation scheme is to allocate reservoirs on to appropriate grids of CaMa-Flood River Map and setting reservoir operation parameters.

## Allocation of Reservoir on CaMa-Flood River Map

The scripts to allocate reservoirs are prepared in $(CaMa-Flood)/map/src/src\_param/ directory.

#### (1) Input data (included in CaMa-Flood package)

List of GRanD reservoirs is available in CaMa-Flood package.

$(CaMa-Flood)/map/data/GRanD\_allocated.csv

Some reservoirs have error or mismatch of the attribute data required for allocation (lat, lon, uparea) compared to the MERIT Hydro river map (hydrography basemap for CaMa-Flood). Thus, we corrected the errors or mismatches by allocation reservoirs on 1-min resolution MERIT Hydro data.

The corrected data is (lat\_alloc, lon\_alloc , area\_alloc). The corrected attribution data is used to allocate GRanD reservoirs on a CaMa-Flood river map. In addition, below attributes are included:

* DamName: Name of the dam
* RiverName: Name of the river
* CAP\_MCM: Reservoir total capacity in Million cubic memer
* YEAR: Construction year
* ALT\_YEAR: Dam alternation year
* RAM\_YEAR: Dam construction year
* ELV\_MASL: Elevation of the dam above mean sea level
* DAM\_HGT\_M: Height of the dam
* lat\_ori, lon\_ori, area\_ori: original location attribute

テーブル

自動的に生成された説明

Example of GRanD\_allocated.csv file.

#### (2) Allocate reservoirs on a CaMa-Flood river map

Please go to your working map directory (e.g. map/glb\_15min/). Then copy map/src/src\_param/ directory to your working map directory. Then, please go to src\_param/ directory in your map directory. Compile the Fortran90 source code by make.

```

% cd map/glb\_15min

% cp -r ../src/src\_param .

% cd src\_param/

% cd make all

```

Then, edit t02-alloc\_dams.sh , and execute it. You can change the input dam list and output file names.


```

% vi t02-alloc\_dams.sh

```

There are two output files in default setting.

* GRanD\_river.txt: Dams allocated on CaMa-Flood river map, reservoir operation applied.
* GRanD\_small.txt: Dams too small to be allocated on CaMa-Flood river map.



Example of GRanD\_river.txt file.

Note; Detailed methodology for allocating reservoirs is explained in the manual of AllocateRiverGauge package.

### Setting Reservoir Operation parameters

#### Working location

Please go to your working map directory (e.g. map/glb\_15min/). Then copy map/src/src\_dam/ directory to your working map directory.

```

% cd map/glb\_15min

% cp -r ../src/src\_dam .

% cd src\_dam/

```

#### Input data for setting reservoir operation parameters

Then, please check the s00-link.sh script, and prepare the required input data for CaMa-Flood reservoir operation scheme.

##### [2a] DAMLIST: List of dams to be allocated

Please prepare the list of dams to be allocated on the CaMa-Flood river map

default: DAMLIST=${MAPDIR}/GRanD\_river.txt

##### [2b] NATDIR: Naturalized simulation output directory

You first need to execute “no reservoir” simulation to estimate 100-year return-period discharge, to estimate flood discharge to start flood control operation. Please specify the location of the naturalized simulation data as NATDIR in s00-link.sh.

It is recommended that “no reservoir” is run with the same runoff forcing data and same river map data as “with reservoir” simulation to keep the consistency of the reservoir parameters. The python script in the current reservoir operation package assumes the output are in plain binary format with 1day time step. Output should be plain binary, and outflwYYYY.bin should be saved. It’s better to have ~30 years of simulations.

Note; the sample script s00-link.sh uses the output of the sample 2-year simulation “test1-glb\_15min”, but this is just for the purpose of checking the reservoir operation scripts are working. It’s better to have 30-year-long simulation to estimate 100-year return-period discharge appropriately.

##### [2c] GRSAD (Global Reservoir Surface Area Dataset)

The reservoir surface area timeseries data is needed to decide normal water volume.

Data can be downloaded below. Please specify the directory where "\*\_intp" files are located as GRSADdir in s00-link.sh script.

<https://dataverse.tdl.org/dataset.xhtml?persistentId=doi:10.18738/T8/DF80WG>

Note: The sample GRSAD data (only 1 dam) is include in CaMa-Flood package

##### [2d] ReGeom data (Global Reservoir Geometry Database)

The reservoir geometry data (area-volume relationship) is needed to decide normal water volume & flood control volume.

Data can be downloaded below. Please specify the directory where "\*.csv" data are located as ReGeomdir in s00-link.sh script.

<https://zenodo.org/record/1322884#.YF1owUj7QW_>

Note: The sample ReGeom data (only 1 dam) is include in CaMa-Flood package

#### Setting reservoir operation parameters

Please edit s01-calc\_damparam.sh script, and execute it.

You need to set SYEAR,EYEAR,DT of the naturalized simulation. (Daily discharge data DT=86400 is assumed)

The Python scripts for (a) calculating annual mean and max discharge at each dam location, (b) calculating 100year discharge at each dam location, (c) estimating normal water storage from satellite data, (d) merging these information into one dam parameter list, (e) finalizing the dam parameter list for use in CaMa-Flood, are sequentially executed.

Temporally output file is saved in the directory set as TAG (default: tmpdat/)

##### [3a] Calculate annual mean and max discharge at each dam location

Annual mean and max discharge at each dam grid are calculated from daily discharge of naturalized simulation by using code script/p01\_get\_annualmax\_mean.py

The output is plain binary data: tmp\_p01\_AnnualMax.bin, tmp\_p01\_AnnualMean.bin

##### [3b] Calculate 100-year discharge at each dam location

100-year return-period discharge is calculated from the annual maximum discharge timeseries calculated in the previous step, by using code script/p01\_get\_annualmax\_mean.py. Plotting Position and L-moments methods are used to estimate Gumbel distribution parameters.

The output is plain binary data: tmp\_p02\_100year.bin

##### [3c] Estimate flood control volume

Then, flood control volume and normal volume are estimated, using satellite-based reservoir storage time-series, using p03\_est\_fldsto\_surfacearea.py. The sum of flood control volume and normal volume is total storage of the reservoir.

We assume reservoir water level is kept at normal water level in wet season when inflow to reservoir is adequate, thus reservoir surface area corresponding to normal water level is frequently observed. Then, we assume the 75th percentile value (pc = 75 in p03 script) of the observed reservoir surface area corresponds to the normal water volume (with calibration and sensitivity check). The 75th percentile water surface area is taken from GRSAD reservoir surface area data, and it is converted to the corresponding volume using reservoir geometry data ReGeom.

The output is CSV file: tmp\_p03\_fldsto.csv

##### [3d] Combine outputs to create reservoir parameter datasts

Dam parameters estimated in previous steps are combined to create dam parameter list file, using p04\_complete\_damcsv.py. For reservoirs which does not have flood control capacity

* Flood discharge (discharge threshold to initiate flood control operation) is 30% of 100-year return-period discharge. If estimated flood discharge is smaller than annual mean discharge, modification is applied (40% of 100-year discharge, or 110% of annual mean discharge)
* For reservoirs with no GRSAD or ReGeom data, flood control storage is given as 37% of total storage.
* The upstream area threshold MINUPAREA is given as an argument to p04 script, and smaller reservoirs are excluded.

The output is CSV file: tmp\_p04\_damparam.csv

##### [3e] Finalize reservoir parameter list

The reservoir parameter list is finalized by adding the number of dams in 1st line of tmp\_p04\_damparam.csv

The name of the finalized reservoir parameter list is given as OUT\_DAMPARAM in s01 script.

Default: OUT\_DAMPARAM="../dam\_param.csv"

グラフィカル ユーザー インターフェイス, アプリケーション, テーブル, Excel

自動的に生成された説明

Sample of finalized reservoir parameter data: dam\_param.csv

If modification of reservoir parameter is needed for your experiment, please edit "../dam\_param.csv"

### Add reservoirs not included in GRanD data

Reservoirs not included in GRanD data can be added by adding their information in input reservoir list data. The sample file is prepared as:

$(CaMa-Flood)/map/data/GRanD\_alloc+Mekong.csv

Please find the latitude, longitude and upstream area of the new reservoir, using MERIT Hydro river map (or CaMa-Flood 1min river map), and specify the data as lat\_MERIT, lon\_MERIT, area\_MERIT), and provide reservoir capacity in million M3 (CAP\_MCM). The other fields can set to undef value (-99). Then please follow the above procedures to allocate reservoirs in CaMa-Flood map, and estimate reservoir parameters.

Note that satellite data to estimate normal water volume is not available for non-GRanD reservoirs. Please set an appropriate value by yourself.

グラフィカル ユーザー インターフェイス, テーブル

自動的に生成された説明

Sample of dams added to input damlist. 5 new dams in Mekong River basin were added.

# Executing simulation with reservoir operation

Sample script to run CaMa-Flood simulation with reservoir operation is prepared in gosh/test6-reservoir\_glb15min.sh.

Reservoir operation scheme can be activated by specifying the reservoir parameter list file. No additional forcing data is needed.

## Namelist for reservoir operation scheme

Please edit the namelist parameters in the gosh script to specify the reservoir scheme setting.

* LDAMOUT=".TRUE." # set to “.TRUE.” to activate reservoir operation (under development)
* CDAMFILE="${FMAP}/dam\_param.csv" # Specify dam parameter list
* CVARSOUT="flddph,outflw,daminf,damsto,rivdph" # Inflow to dam, storage of dam can be outputted.
* LDAMTXT= ".TRUE." # set to “.TRUE.” for text-based reservoir data output
* LDAMH22= ".FALSE." # TRUE to use Hanazaki 2022 dam scheme (not recommended). If set to FALSE, the updated version Yamazaki & Funato scheme is used (recommended).

## Code for reservoir operation scheme

The reservoir operation is activated by LDAMOUT flag. You can check the codes related to reservoir operation by searching this tag in CaMa-Food Fortran90 codes.

#### Basic strategy to represent reservoir operation

Basic strategy to represent reservoir operation in CaMa-Flood is: [1] First, calculate “natural” river discharge using local-inertial equation for all grid cells (including grids with reservoir) by CALL CMF\_CALC\_OUTFLW ; [2] Then, replace the “natural” discharge of the grids with dams, by reservoir operation scheme, by CALL CMF\_DAMOUT\_CALC ; [3] Then, calculate “inflow” at all grid cells, and modify the discharge if water budget error happens by CALL CMF\_CALC\_INFLOW ; [4] Check reservoir operation scheme water balance by CALL CMF\_DAMOUT\_WATBAL.

This calculation flow appears as below in cmf\_ctrl\_physics\_mod.F90.

```

!=== 1. Calculate river discharge

CALL CMF\_CALC\_OUTFLW !! Default: Local inertial

! --- v4.12: damout before pthout for water buget error

IF ( LDAMOUT ) THEN

CALL CMF\_DAMOUT\_CALC !! reservoir operation

ENDIF

! --- Water budget adjustment and calculate inflow

CALL CMF\_CALC\_INFLOW

IF ( LDAMOUT ) THEN

CALL CMF\_DAMOUT\_WATBAL !! reservoir operation

ENDIF

```

#### Reservoir operation module

The code for reservoir operation is prepared as Fortran90 module (cmf\_ctrl\_damout\_mod.F90). The module contains below subroutines.

##### SUBROUTINE CMF\_DAMOUT\_NMLIST

Read Namelist parameters specific for reservoir operation scheme

##### SUBROUTINE CMF\_DAMOUT\_INIT

Initialize reservoir operation scheme.

* Specified reservoir parameter list is read, and parameters for each reservoir is determined.
* Reservoir storage is initialized (using restart file if specified)
* Deactivate bifurcation scheme around the reservoir lake, to avoid instability and un-expected water leakage from reservoir

##### SUBROUTINE CMF\_DAMOUT\_CALC

Primary code for calculating reservoir operation.

First, the inflow to the reservoir grid is replaced by using kinematic-wave equation (CALL UPDATE\_INFLOW). This is needed to avoid “storage buffer effect” (unexpected rise of water level in upstream of reservoir, due to imperfect representation of reservoir topography and storage-stage relationship).

Then, reservoir outflow is calculated following the storage and inflow condition of each reservoir.

In CaMa-Flood v4.13, two reservoir operation schemes are prepared.

* LDAMH22=.TRUE. for Hanazaki et al. 2022 scheme. There was some issues in this scheme, so we don’t recommend to use this.
* LDAMH22=.FALSE. for Yamazaki & Funato (in prep) scheme. We made some updated to increase the stability and reality of Hanazaki 2022 scheme. The description paper is in preparation now.

##### SUBROUTINE CMF\_DAMOUT\_WATBAL

Water budget error specific for reservoir operation scheme is checked. Calculated water budget is written in the log file of CaMa-Flood simulation (log\_CaMa.txt). Please confirm that the water budget error is adequately small (smaller than the order of rounding error).

CMF::TIME\_NEXT: 1 0 1440 86400.0000

Strt of Tstep: KMIN, IYYYYMMDD, IHHMM 0 20010101 0

End of Tstep: KMINNEXT, JYYYYMMDD, JHHMM 1440 20010102 0

ADPSTP: NT= 259 86400.00 334.67 333.59

CMF::DAM\_CALC: DamMiss at all dams: -4.3612718582153323E-013

2001/01/01\_00:05 1 flx: 5138.649 5138.410 5138.662 -0.641E-12 10.009 10.247 stg: 5138.662 5138.662 -0.00 1537.359 3601.302 1639.659


CMF::DAM\_CALC: DamMiss at all dams: 8.4400177001953130E-014

2001/01/01\_00:11 2 flx: 5138.662 5138.425 5138.677 0.307E-11 10.008 10.245 stg: 5138.677 5138.677 -0.00 1537.385 3601.292 1639.725

##### SUBROUTINE CMF\_DAMOUT\_WRTE

If LDAMTXT= ".TRUE.” , the time series of the DamStorage, DamInflow, DamOutflow of each reservoir is saved.

The output text file name is ‘damtxt-(YYYY).txt”



Example of damout-(YYYY).txt. In addition to the timeseries of DamStorage, DamInflow, DamOutflow, basic dam parameters (DamID, TotalVolume & Normal Volume [Million m3], Upstream area [km2], Flood Discharge and Normal Discharge [m3/s]) are written in the top pf the text file.